.. currentmodule:: machine
.. _machine.UART:

class UART -- duplex serial communication bus
=============================================

UART implements the standard UART/USART duplex serial communications protocol.  At
the physical level it consists of 2 lines: RX and TX.  The unit of communication
is a character (not to be confused with a string character) which can be 8 or 9
bits wide.

UART objects can be created and initialised using::

    from machine import UART

    uart = UART(3, 9600)                         # init with given baudrate
    uart.init(9600, bits=8, parity=None, stop=1) # init with given parameters

Bits can be 7, 8 or 9. Stop can be 1 or 2. With *parity=None*,
only 8 and 9 bits are supported.  With parity enabled, only 7 and 8 bits
are supported.

A UART object acts like a :std:term:`stream` object and reading and writing is done
using the standard stream methods::

    uart.read(10)       # read 10 characters, returns a bytes object
    uart.read()         # read all available characters
    uart.readline()     # read a line
    uart.readinto(buf)  # read and store into the given buffer
    uart.write('abc')   # write the 3 characters

Constructors
------------

.. class:: UART(id, ...)

   Construct a UART object of the given id.

Methods
-------

.. method:: UART.init(baudrate=9600, bits=8, parity=None, stop=1, \*, ...)

   Initialise the UART bus with the given parameters:

     - *baudrate* is the clock rate.
     - *bits* is the number of bits per character, 7, 8 or 9.
     - *parity* is the parity, ``None``, 0 (even) or 1 (odd).
     - *stop* is the number of stop bits, 1 or 2.

   Additional keyword-only parameters that may be supported by a port are:

     - *tx* specifies the TX pin to use.
     - *rx* specifies the RX pin to use.
     - *rts* specifies the RTS (output) pin to use for hardware receive flow control.
     - *cts* specifies the CTS (input) pin to use for hardware transmit flow control.
     - *txbuf* specifies the length in characters of the TX buffer.
     - *rxbuf* specifies the length in characters of the RX buffer.
     - *timeout* specifies the time to wait for the first character (in ms).
     - *timeout_char* specifies the time to wait between characters (in ms).
     - *invert* specifies which lines to invert.

         - ``0`` will not invert lines (idle state of both lines is logic high).
         - ``UART.INV_TX`` will invert TX line (idle state of TX line now logic low).
         - ``UART.INV_RX`` will invert RX line (idle state of RX line now logic low).
         - ``UART.INV_TX | UART.INV_RX`` will invert both lines (idle state at logic low).

     - *flow* specifies which hardware flow control signals to use. The value
       is a bitmask.

         - ``0`` will ignore hardware flow control signals.
         - ``UART.RTS`` will enable receive flow control by using the RTS output pin to
           signal if the receive FIFO has sufficient space to accept more data.
         - ``UART.CTS`` will enable transmit flow control by pausing transmission when the
           CTS input pin signals that the receiver is running low on buffer space.
         - ``UART.RTS | UART.CTS`` will enable both, for full hardware flow control.

   .. note::
     It is possible to call ``init()`` multiple times on the same object in
     order to reconfigure  UART on the fly. That allows using single UART
     peripheral to serve different devices attached to different GPIO pins.
     Only one device can be served at a time in that case.
     Also do not call ``deinit()`` as it will prevent calling ``init()``
     again.

   .. note::
     It is possible to call ``init()`` multiple times on the same object in
     order to reconfigure  UART on the fly. That allows using single UART
     peripheral to serve different devices attached to different GPIO pins.
     Only one device can be served at a time in that case.
     Also do not call ``deinit()`` as it will prevent calling ``init()``
     again.

.. method:: UART.deinit()

   Turn off the UART bus.

   .. note::
     You will not be able to call ``init()`` on the object after ``deinit()``.
     A new instance needs to be created in that case.

.. method:: UART.any()

   Returns an integer counting the number of characters that can be read without
   blocking.  It will return 0 if there are no characters available and a positive
   number if there are characters.  The method may return 1 even if there is more
   than one character available for reading.

   For more sophisticated querying of available characters use select.poll::

    poll = select.poll()
    poll.register(uart, select.POLLIN)
    poll.poll(timeout)

.. method:: UART.read([nbytes])

   Read characters.  If ``nbytes`` is specified then read at most that many bytes,
   otherwise read as much data as possible.

   Return value: a bytes object containing the bytes read in.  Returns ``None``
   on timeout.

.. method:: UART.readinto(buf[, nbytes])

   Read bytes into the ``buf``.  If ``nbytes`` is specified then read at most
   that many bytes.  Otherwise, read at most ``len(buf)`` bytes.

   Return value: number of bytes read and stored into ``buf`` or ``None`` on
   timeout.

.. method:: UART.readline()

   Read a line, ending in a newline character.

   Return value: the line read or ``None`` on timeout.

.. method:: UART.write(buf)

   Write the buffer of bytes to the bus.

   Return value: number of bytes written or ``None`` on timeout.

.. method:: UART.sendbreak()

   Send a break condition on the bus. This drives the bus low for a duration
   longer than required for a normal transmission of a character.

.. method:: UART.flush()

   Waits until all data has been sent. In case of a timeout, an exception is raised. The timeout
   duration depends on the tx buffer size and the baud rate. Unless flow control is enabled, a timeout
   should not occur.

   .. note::

       For the rp2, esp8266 and nrf ports the call returns while the last byte is sent.
       If required, a one character wait time has to be added in the calling script.

   Availability: rp2, esp32, esp8266, mimxrt, cc3200, stm32, nrf ports, renesas-ra

.. method:: UART.txdone()

   Tells whether all data has been sent or no data transfer is happening. In this case,
   it returns ``True``. If a data transmission is ongoing it returns ``False``.

   .. note::

       For the rp2, esp8266 and nrf ports the call may return ``True`` even if the last byte
       of a transfer is still being sent. If required, a one character wait time has to be
       added in the calling script.

   Availability: rp2, esp32, esp8266, mimxrt, cc3200, stm32, nrf ports, renesas-ra

Constants
---------

.. data:: UART.RX_ANY

    IRQ trigger sources

    Availability: WiPy.
